How to install – Panel Glides

Tools you will need –

• A Cordless Drill or Screwdriver,

With a Philips head.

The Brackets have to be installed onto a hard surface, such as your architrave or window frame. If installed to any other kind of surface you will need to use wall plugs or anchors as specified below to ensure the blind is held firmly in place.

**For installing onto Plaster walls**

Use 10mm Wall Anchors (available in our store)

**For installing onto Timber**

Pre-drill holes and use the included screws.

For installing onto Concrete walls, stone & solid walls

Use a masonry drill and appropriate plugs, wall anchors Or screws. (Available in our store)

**Positioning the Brackets – ensure they are in a straight line**

The brackets of these blinds need to be mounted approx. 100mm’s in from each end of the track. Make sure that the brackets will not interfere with the operation of the panel blind itself. Install extra brackets if required evenly across the blind, no more than 800mm gap between each of them.

**Mounting Blind**

Lay your panels out on a flat, clean surface. Each panel has a clasp at the top that just pops into the guide and allows it to hang.

**Child Safety**

It is the responsibility of the person installing the blinds to make sure that child safety devices supplied by us are installed when you install the blind. All warning tags are to remain on the blinds.

Due to the high risk of child/pet strangulation please ensure that cords are maintained and kept out of reach of danger.