How to install – timber venetians

|  |  |
| --- | --- |
| Tools you will need: | |
| Cordless Drill with Phillips Head drill bit |  |

The Brackets have to be installed onto a hard surface, such as your architrave or window frame. If installed to any other kind of surface you will need to use wall plugs or anchors as specified below to ensure the blind is held firmly in place.

**For installing onto Plaster walls**

Use 10mm Wall Anchors (available in our store)

**For installing onto Timber**

Pre-drill holes and use the included screws.

For installing onto Concrete walls, stone & solid walls

Use a masonry drill and appropriate plugs, wall anchors Or screws. (Available in our store)

**Positioning Brackets**

Space the support brackets out evenly. Making sure that there is a bracket at no more than 800mm apart and that the brackets are fastened in a straight line

**Mounting Blind** Open the hinged gate of the End Bracket and secure into position using the provided 20mm self-tapping screws. **Face Mount -** use the screw-hole positions at the back of the bracket plate. **Recess Mount -** use the screw-hole positions at the top of the plate. Mount the Central Support Bracket in the same manner. Slide the head rail box into the brackets and close the gates on the end brackets left and right.

To operate the blind, make sure the slats are in the open position before being raised or lowered. Failure to do so may result in damaging the blind and voiding the warranty.

**Attaching the Valance** Place the back of your valance clips into the channel on the back of the valance at a 90 degree angle and twist them to the upright position to lock them in place. If you have a face fit timber Venetian you will need to slide the returns in the channel on the ends of the valance.

**Child Safety**

It is the responsibility of the person installing the blinds to make sure that child safety devices supplied by us are installed when you install the blind. All warning tags are to remain on the blinds.

Due to the high risk of child/pet strangulation please ensure that cords are maintained and kept out of reach of danger.