How to install – Vertical Blinds

Tools you will need:

Cordless drill with a Phillip’s head drill bit

Tape measure

|  |  |
| --- | --- |
| Step ladder (if windows are high) |  |

The Brackets have to be installed onto a hard surface, such as your architrave or window frame. If installed to any other kind of surface you will need to use wall plugs or anchors as specified below to ensure the blind is held firmly in place.

**For installing onto Plaster walls**

Use 10mm Wall Anchors (available in our store)

**For installing onto Timber**

Pre-drill holes and use the included screws.

For installing onto Concrete walls, stone & solid walls

Use a masonry drill and appropriate plugs, wall anchors Or screws. (Available in our store)

 **Positioning Brackets**

Space the support brackets out evenly. Making sure that there is a bracket at no more than 800mm apart and that the brackets are fastened in a straight line

**Mounting Blind**

**Child Safety**

It is the responsibility of the person installing the blinds to make sure that child safety devices supplied by us are installed when you install the blind. All warning tags are to remain on the blinds.

Due to the high risk of child/pet strangulation please ensure that cords are maintained and kept out of reach of danger.