How to install roller blinds

Tools you will need –

• A Cordless Drill or Screwdriver,

With a Philips head.

The Brackets have to be installed onto a hard surface, such as your architrave or window frame. If installed to any other kind of surface you will need to use wall plugs or anchors as specified below to ensure the blind is held firmly in place.

**For installing onto Plaster walls**

Use 10mm Wall Anchors (available in our store)

**For installing onto Timber**

Pre-drill holes and use the included screws.

For installing onto Concrete walls, stone & solid walls

Use a masonry drill and appropriate plugs, wall anchors Or screws. (Available in our store)

**Positioning the Brackets – ensure they are in a straight line**

The brackets will either be in the recess of your window or the face of your window depending on where you measured.

If they are on the face position the brackets at each end of the window frame where you measured from and secure using the screws in your package. The chain bracket will be installed on the side in which you asked the control to go on.

If they are in the recess secure the chain drive bracket hard up to the recess, remember where you secure your brackets is where your blind will sit so keep this in mind. The pin end is then secured a few millimetres in from the other end. Your brackets have two options for fixing, one is for the top securing or the side securing, this option is up to you and where you are able to secure it best.

**Mounting Blind**

Pop the blind into the chain end first, you may need a second person for this if your blind is large.

Ensure the chain end is hanging from your bracket so that it can be operated freely and looks like it is draped over the roll. At the other end is a pin depress the pin so that it will enable you to pop the end in the pin end easily. Once in position and you let go of the pin it will pop out and hold the blind securely.

**Child Safety**

It is the responsibility of the person installing the blinds to make sure that child safety devices supplied by us are installed when you install the blind. All warning tags are to remain on the blinds.

Due to the high risk of child/pet strangulation please ensure that cords are maintained and kept out of reach of danger. It is a requirement of the child safety law.